LSI-11 Bus Signals

Component Side Solder Side

BIRQ6 L BDAL16 L BDAL17 L SSPARE1

GROUND MSPAREA

GROUND BDMR L

SSPARE3

BHALT L BREF L +12V or +5V Battery GROUND PSPARE1 +5V Battery

BIRQ5 L

connected to AK1

BA

AA AB AC AD AE AF AH AJ AK AL AM AN AP AR AS AT AU AV

1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1

BB BC BD DE BF BH BJ BK BL BM BN BP BR BS BT BU BV

1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1

BDCOK H BPOK H BDAL18 L (or SSPARE4) BDAL19 L (or SSPARE5) BDAL20 L (or SSPARE6) (or SSPARE7)

BDAL21L SSPARE8 GROUND MSPAREB MSPAREB

MSPAREA not bussed, but

not bussed, but connected to BK1 GROUND BSACK L BIRQ7 L BEVNT L 12V Battery GROUND PSPARE2 no connection

no connection

BA

AA AB AC AD AE AF AH AJ AK AL AM AN AP AR AS AT AU AV

BB BC BD DE BF BH BJ BK BL BM BN BP BR BS BT BU BV

2 2 2 2 2 2 2 2 2 2 2 2 2 2 2 2 2 2

2 2 2 2 2 2 2 2 2 2 2 2 2 2 2 2 2 2

+5V POWER

+5V POWER

GROUND +12V POWER BDOUT L BRPLY L BDIN L BSYNC L BWTBT L BIRQ4 L BIAKI L BIAKO L BBS7 L BDMGI L BDMGO L BINIT L BDAL0 L BDAL1 L

+5V POWER

GROUND +12V POWER BDAL2 L BDAL3 L BDAL4 L BDAL5 L BDAL6 L BDAL7 L BDAL8 L BDAL9 L BDAL10 L BDAL11 L BDAL12 L BDAL13 L BDAL14 L BDAL15 L

SRUN (or SSPARE2)

-12V (Optional)

-12V (Optional)